GoeMobile

The GWDG provides the network infrastructure for the University of Göttingen, the Max-Planck-Institute and partly also for other scientific institutes in and around Göttingen. This includes the wireless LAN GoeMobile, which is integrated into the main network infrastructure GÖTNET. It provides mobile users with internet access in many locations and can also be used for lectures and conferences.

Available WLANs

In the Göttingen WLAN the following networks (SSIDs) are available:

eduroam (recommended)

Available on all sites with 802.11 b/g and 802.11n (5 GHz), encrypted with WPA2. Login with an eduroam-compatible account.

GoeMobile

Available on all sites unencrypted with 802.11 b/g and 802.11n (5 GHz) for fast access with up to 300 MBit/s. Login via the WebPortal (not within the University clinic) and encryption possible with VPN. 802.11n will be chosen automatically from your WLAN device or has to be chosen manually in the program of your driver if necessary.

GoeMobile-vpnonly

This WLAN (802.11 b/g) is intended for devices which have problems with the WebPortal login. In this unencrypted WLAN login is only possible through VPN. This network is available at all sites where GoeMobile is available (except for the UKG). The SSID is hidden and must be preselected in the device.

Requirements

An account with the GWDG, with studIT or with one of the institutes taking part in the DFN-Roaming and compliance with the terms of use.

Website:

http://www.goemobile.de

tag>WLAN goemobile wireless radio network GWDG